

Wall

For fixed wall temp:

For adiabatic wall:

At BL edge:

,